============================================================
 VX-3000 Setting Software Ver.5.30.0
                                               Jun 13, 2023
============================================================

ReadMe file


Thank you for downloading the TOA's VX-3000 Setting Software Ver.5.30.0.

The VX-3000 Setting Software Ver.5.30.0 ("This software" herein)
is designed for exclusive use with the TOA's VX-3000 Series. 

This ReadMe file contains the following information.

1. About this software
2. Installing this software
3. How to confirm software installation completion
4. Update history


1. About this software
------------------------------------------------------------
This software is a program used to perform VX-3000 system settings and maintenances.


2. Installing this software
------------------------------------------------------------
First, be sure to exit all software programs before installing this software.
Then, execute the "VX-3000_setup.msi" file contained in the same folder as this software.
As the installer is activated, follow the on-screen instructions.
For details, refer to the software instruction manual
that can be obtained at our product information download site.
(https://www.toa-products.com/international/)


3. How to confirm software installation completion 
------------------------------------------------------------
The updated software of version 5.30.0 runs after installation completion.
Selecting "Help" from the menu bar after starting the installed
VX-3000 software displays the version information.
Confirm that "Ver.5.30.000" is displayed. 


4. Update history
------------------------------------------------------------
-Ver.5.30.0
*RM-300X and RM-200SF cannot use "Priority last" when the talk button is in PTT mode.
*Modification of wording in English, German and French.


-Ver.5.20.0
*Compatible with RM-500
*"EMG enable operation" was added to the content 3 of the "Emergency broadcast pattern start"
*Improvement of impedance value display accuracy


-Ver.5.10.0
The added functions are as follows:
*Compatible with VX-3000PM, VX-3000CT and VX-300LO
*Sleep mode
*Chime sound source to audio source type of general broadcast pattern setting
*Related control output to VX-3004F and VX-3008F audio output settings


-Ver.5.1.0
The fixed functions are as follows:
*Daily program contents cannot be changed in advanced end user mode


-Ver.5.0.0
The added functions are as follows:
*Access level setting for each user
*Simple setting mode
*Timer setting
*Change the scale of impedance value to ohm
*Activate control output when selecting zones
*Set emergency mode when activating emergency warning broadcast
*Notification buzzer for disablement of EMG control from CIN
*Control output interlocked with emergency broadcast state
*Function pulldown menu layering of event setting
*Expand the number of emergency sequence phases up to 30
*TALK key event separation in emergency/general mode 
 when emergency RM or emergency/general RM is used
*Added every 2 hours to battery check interval setting


-Ver.4.0.0
The added functions are as follows:
*Supported system combination function


-Ver.3.1.0
The added functions are as follows:
*Function that can select the power supply voltage specification with 230V and 100V
*When the power supply voltage specification is 100 V, the function that can select the 100V specification amplifier (VX-012DA-2, VX-024DA-2, VX-036DA-2)
*Enhancements for receiving unit configuration


-Ver.3.0.0
The added functions are as follows:
*Email functions for fault detections
*Modbus Protocol
*40 units expansion
*EMG silence function
*Pre zone selections for Emergency EV message
*Selectable for PAGING or PAGING&BGM broadcasting during AC-power OFF
*EV message 8 words binding 
*Individual zone assignment for TALK key
*Standby AMP settings when a DS strides some areas
*EMG ACK function
*Disable function for EMG activation by control inputs
*NO/NC settings for EMG events
*Several RM-200SF can be connected to a RS-LINK
*EV sequence phase time : 10 sec. step setting
*Language in German, French and Japanese
*Improve the procedure for unit detection, receiving unit configuration and maintenance system detection
*Improve the error indications for setting data uploading and downloading failures
*Output setting data as CSV file


-Ver.2.0.0
The added functions are as follows:
*Enhancements for PA functions
*Enhancements for EVAC functions
*Enhancements for Fault detect functions
*Remote Protocol
*Network Audio Protocol

------------------------------------------------------------
(c) 2018 TOA Corporation.